SRI KRISHNA COLLEGE OF TECHNOLOGY

COIMBATORE

DEPARTMENT OF ELECTRONICS AND COMMUNICATION ENGINEERING

IBM NALAIYA THIRAN

ASSIGNMENT-1

TEAM LEADER: SWEDHA D

TEAM MEMBER: SANGAMITRA SU

SOWMIYA K

VIJAYA DHARSHINI R

SMART HOME AUTOMATION-DOOR BUZZER

CODE:

int trig=2; int echo=3; int buzzer=10; int time; int distance; void setup()

{

Serial.begin(9600); pinMode(trig,OUTPUT); pinMode(echo,INPUT); pinMode(buzzer,OUTPUT);

}

void loop()

{

digitalWrite(trig,HIGH);

delayMicroseconds(10); digitalWrite(trig,LOW); time=pulseIn (echo,HIGH); distance=(time\*0.034)/2; if(distance<=10)

{

Serial.println("DOOR OPEN");

Serial.print("distance:"); Serial.println(distance); digitalWrite(buzzer,HIGH); delay(500);

}

else

{

Serial.println("DOOR CLOSED");

Serial.print("distance:"); Serial.println(distance); digitalWrite(buzzer,LOW); delay(500);

}

}

